|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ITEM** | **PRODUCT** | **DOSAGE**  **RATE** | **PPE REQUIRED** | **METHOD** |
| **Vacuum Packing Machine**  ***Must be cleaned prior to and after each use*** | Oasis Pro 20 | 20 ml via dispenser per 600 ML trigger spray | Nitrile/Latex-free Gloves EN374 for prolonged use | **Interior**  Remove the insert plate. Remove any food debris. Thoroughly clean the lid, the silicon strip, the counter bar and interior base, sides and walls of the vacuum chamber with a clean damp cloth and Oasis Pro 20 solution.  Spray all surfaces with Oasis Pro 20 sanitising solution and leave for one minute. Then rinse and wipe dry with paper towel.  Thoroughly clean all surfaces of the insert plate with a clean damp cloth and Oasis Pro 20 solution.  Spray insert plate surfaces with Oasis Pro 20 sanitising solution and leave for one minute. Then rinse and wipe dry with paper towel. Replace the insert plate in position.  **Exterior**  Thoroughly clean all of the exterior surfaces with a clean damp cloth and Oasis Pro 20 solution. Spray surfaces with Oasis Pro 20 sanitiser and leave for one minute. Then rinse and wipe dry with paper towel. |