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Workplace Safety Management System
	RA-LE
	Risk Assessment

Leisure Services

	Unit Name and number
	

	Risk Assessment Completed
	Name:

Date:
	Signed:

	1st review
	Name:

Date:
	Signed:

	2nd review
	Name:

Date:
	Signed:

	3rd review
	Name:

Date:
	Signed:



Note - Risk assessments must be reviewed every 3 years, whenever there is a significant change in the activity, and following any incident involving the activity. Risk assessments must be retained for a period of 6 years.

	Step 1 - What are you already doing to control the risk?

	Identify all of the Essential Risk Assessments you have completed for your unit or business operation
by ticking the boxes below. 
(Those which are absolute mandatory completion have already been ticked for you).

	R ES00 Workplace Risk Assessment  
R ES01 Fire Risk Assessment  
R ES02 First Aid Needs Assessment
R ES03 Floor Safety Risk Assessment
R ES04 Manual Handling Activity Filter
£ ES04a Lifting and Carrying Risk Assessment
£ ES04b Pushing and Pulling Risk Assessment 
R ES05 COSHH Product Inventory
R ES06 PPE Assessment  
£ ES06a PPE Issue Form
R ES07 PAT Testing
R ES08 Work Equipment Inspection 
£ ES08a Work Equipment Inspection Register  
	
	R ES09 DSE Risk Assessment  
£ ES09a DSE User Assessment Form
£ ES09b DSE User Risk Assessment
£ ES10 New and Expectant Mothers Risk Assessment 
£ ES11a Young Person’s Risk Assessment (16-17 years)
£ ES11b Young Person’s Risk Assessment (<16 years)
£ ES12 Lone Workers Risk Assessment
£ ES12a Lone Workers Workplace Checklist
£ ES13 Workplace Stress Risk Assessment
£ ES13a Stress Talking Toolkit
£ ES14 Gas Safety Risk Assessment 
R ES15 Violence at Work Risk Assessment



	Step 2 - Workplace Hazards, Risks and Control Measures

	Review this section of the risk assessment and ensure everything detailed below is aligned to your unit.
Document any additional hazards and control measures you have identified in the blank section provided.

	What are the hazards?
	Who might be harmed?
	How might they be 
harmed?
	What additional actions must be taken to control the risk?

	Changing rooms and showers

· Wet floors and pooling water.
· Bacterial/viral/
fungal
contamination
· Damaged lockers, benches, flooring or hooks.
· Electrical equipment such as hair dryers

	Leisure centre users
Compass employees
Contractors


	Severe injuries/broken or fractured bones/bruising/
cuts/sprains/strains from slips in showers or on wet/slippery floors

Fungal/viral/bacterial Infections as a result of inadequate hygiene and cleaning

Impact injuries/cuts/splinters as a result of damaged lockers, benches, hooks etc.
Electric shock/burns from use of damaged or poorly maintained equipment 

	· Facilities are maintained in a safe condition and any damage to structure/equipment reported
· Regular inspections of electrical systems and equipment conducted to identify and address potential issues
· Unsafe electrical equipment is removed from use
· Where appropriate, slip-resistant mats are used to reduce the risk of slips
· Adequate drainage to avoid water pooling.
· Signage promoting good personal hygiene displayed
· Daily cleaning and sanitation protocols in place.

	Gymnasium
 
· Malfunctioning equipment
· Poorly maintained equipment
· Incorrect use of equipment
· Gym equipment poorly arranged or located 
· Wet floors as a result of sweat or spills 
· Bacterial/viral/
fungal contamination 
· Inadequate ventilation increasing risk of airborne illnesses 
· Incorrect lifting techniques
· Overexertion
· Ill health as a result of existing health conditions or contra-indications including: 
· low or high blood pressure
· cardiovascular issues 
· diabetes
· seizures
· pregnancy
· use of certain medications
· electrical gym equipment

	Leisure centre users
Compass employees
Contractors

	Severe or fatal injuries/broken or fractured bones/entrapment injuries/bruising/cuts/sprains/
strains from:
· Use of malfunctioning or poorly maintained equipment
· User lack of knowledge using gym equipment
· Slips, trips or falls from wet floors, sweat or spills.
· Collisions, trips & falls due to poor equipment spacing and user overcrowding

Collapse/dehydration/ill health due to:
· Overexertion or poor lifting techniques resulting in accident and injury. 
· Persons using equipment with existing health conditions or contra-indications

Illness or infection due to:
· Inadequate hygiene, cleaning and sanitation.
· Inadequate ventilation.



	· All gym equipment supplied to British standards BS EN 957
· Contracts in place for regular maintenance of equipment
· Members to complete a health declaration to identify any health conditions or contra-indications
· Regular checks of equipment carried out, and defects reported
· Defective equipment taken out of use
· Flooring regularly inspected and maintained to address slip hazards and wear and tear 
· Prominent signage displayed advising on safe and hygienic use of equipment
· Regular cleaning and sanitation implemented
· Walking the floor checks in place at regular intervals
· Areas kept well-organized and free from clutter and obstructions
· Designated storage areas for gym bags and personal items provided
· Adequate lighting provided throughout the gym 
· Members offered an induction prior to first use
· Persons under the age of 18 not permitted to use gym equipment





	Tennis Courts

· Debris, cracks, poorly maintained or uneven surfaces.
· Weather-related issues.
· Poorly maintained or damaged facilities/equipment
· Obstructions hazards on tennis court access route
· Inadequate lighting
	Leisure centre users
Compass employees
Contractors

	Severe injuries/broken or fractured bones/bruising/
cuts/sprains/strains as a result of slips, trips and falls caused by:
· Uneven/rough ground, or debris (such as leaves or moss)
· Wet/slippery ground
· Poor lighting

Heat stroke/exhaustion from exertion in extreme heat.

Impact injuries from falling branches etc from nearby trees.

	· Tennis courts, surrounding areas and access routes well maintained
· Tennis courts, surrounding areas and access routes kept free of debris, moss, and other obstructions
· Equipment, including rackets, nets, and posts, well maintained and regularly inspected for damage
· Facilities closed in severe weather, such as strong winds, heavy rain, thunderstorms and outside of daylight hours
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· Pool water
· Slips, trips & falls from slippery surfaces
· Electrical hazards from poolside equipment
· Poor water quality
· Pathogens from swimming pool users
· Entrapment hazards from poorly designed/ maintained drain covers
· Debris in water and surrounding areas
· Excessive bather load resulting in:
· Reduced visibility
· Poor water quality
· Collisions

	Leisure centre users
Compass employees
Contractors


	Severe or fatal injuries/broken or fractured bones/bruising/cuts
/sprains/strains from
· Slips trips and falls are a result of slippery surfaces due to water splashes/poor housekeeping
· Collisions during activities in the pool

Drowning or serious injury due to inability to swim, ill health or dangerous activity/horseplay.

Electrocution or electrical burns from faulty or improperly installed electrical systems/equipment.

Entrapment injuries and drowning due to strong suction from the water circulation system and poorly designed/maintained/
missing drain covers.

Microbiological contamination of pool water and surrounds with parasites/viruses/bacteria/fungi/
algae causing gastrointestinal/skin illness/infections as a result of:
· Poor water quality due to pour water quality management
· Inadequate hygiene standards
· Infected users
· Failing pool plant as a result of poor maintenance
· Contamination of water as a result of faecal incidents or vomiting


	· Documented Pool Safety Operating Procedures (PSOP) established and available. PSOP includes Normal Operating Plan (NOP) and Emergency Action Plan (EAP)
· All poolside electrical equipment appropriate for the area. All electrical components installed by a licensed electrician
· Regular inspections of electrical systems and equipment conducted to identify and address potential issues
· RCDs (Residual Current Devices) used for all electrical equipment near the pool to prevent electrocution
· Pool area is covered by CCTV, which is monitored at all times the pool is open
· Emergency panic buttons available at poolside
· Maintained safety and emergency equipment including rescue equipment (poles, throw bags, buoyancy aids), first aid kits and AEDs available poolside
· Handrails are installed at steps into the pool
· Depth of the pool is clearly marked
· Anti-entrapment drain covers that comply with safety standards installed
· Documented plan in place for responding to incidents faecal/vomit incidents and staff trained on procedures
· Regular inspection and maintenance of pool drains and suction outlets to ensure they are functioning correctly
· Regular checks and clean of filters to prevent clogs
· Regular cleaning of pool via sweeping, skimming and vacuuming
· Employees wear slip-resistant shoes
· Walking the floor checks in place at regular intervals
· Bather load calculated
· Bather attendance monitored and maximum bather load not exceeded
· Access to the pool is restricted when the pool is closed
· Poolside is maintained tidy and organised, without obstructions, and as dry as possible
· Emergency exits are kept clear
· Safe water quality maintained
· Regularly testing of pool water to monitor water quality
· Corrective actions implemented when required to ensure pool water quality is maintained
· At all times the pool is in operation there is a competent person on site, who can deal with any problems relating to pool plant, water treatment, equipment and other emergencies
· Employees are trained in general pool safety, pool operating procedures and the EAP
· At all times the pool is open, a trained First Aider is available
· Documented cleaning schedule in place
· Opening/closing checks and weekly safety reviews completed, and corrective actions taken where required
· Pool rules and safety signage displayed in changing rooms and poolside
· Users’ behaviour is monitored and corrected where required
· Encourage bathers to shower before entering the pool facilities
· Persons considered being under the influence of drink/drugs are not permitted to access the swimming pool areas and are removed where required
· Children under the age of 2, and those not potty trained must wear swim nappies
· All children under the age of 16yo must be accompanied by an adult
· Children under 8 require an adult in the water with them
· No shoes to be permitted to be worn by users or other persons accessing in the pool area or overshoes to be provided and worn
· The use of glass is not permitted in the pool area


	[bookmark: _Hlk212800780]Spa Pool/Jacuzzi:

· Pool water
· Wet/slippery flooring
· Electrical components
· Poor water quality
· Pathogens from users
· Legionella
· Ill health as a result of existing health conditions or contra-indications including: 
· low or high blood pressure
· cardiovascular issues 
· diabetes
· seizures
· pregnancy
· use of certain medications 





	Compass employees
Visitors/guests

	Severe or fatal injuries/broken or fractured bones/bruising/cuts
/sprains/strains from
· Slips trips and falls due to slippery surfaces/water splashes/poor housekeeping.

Microbiological contamination of pool water and surrounds with parasites/viruses/bacteria/fungi/ causing gastrointestinal/skin illness/infections as a result of:
· Poor water quality due to inadequate water treatment
· Poor hygiene standards
· Infected users
· Failing pool plant as a result of poor maintenance

Legionella infection as a result of poorly managed spa pool systems. 

Collapse/dehydration/illness due to overheating, prolonged exposure to hot water underlying health conditions or contra-indications. 

Severe injuries or drowning as a result of entrapment.

Electrocution or electrical burns from faulty or improperly installed electrical systems/equipment.

	· Documented Pool Safety Operating Procedures (PSOP) established and available. PSOP includes Normal Operating Plan (NOP) and Emergency Action Plan (EAP)
· Legionella written scheme of control specific to the spa pool system and facilities is in place
· Regular inspections of electrical systems and equipment conducted to identify and address potential issues
· RCDs (Residual Current Devices) used for all electrical equipment near the pool to prevent electrocution
· Handrails are installed at steps into the pool.
· Bather load calculated
· Bather attendance monitored and maximum bather load not exceeded
· Spa pool is covered by CCTV, which is monitored at all times the pool is open
· Emergency panic buttons available at poolside
· Properly maintain drains and moving parts to reduce risks of hair and body parts entrapment
· Regular inspection and maintenance of pool drains and suction outlets to ensure they are functioning correctly
· Anti-entrapment drain covers that comply with safety standards installed
· Documented plan in place for responding to faecal/vomit incidents and staff trained on procedures
· At all times the pool is in operation there is a competent person on site, who can deal with any problems relating to pool plant, water treatment, equipment and other emergencies
· Employees are trained in general pool safety, pool operating procedures and the EAP
· At all times the pool is open, a trained First Aider is available
· Safe water quality maintained
· Regularly testing of pool water to monitor water quality
· Corrective actions implemented when required to ensure pool water quality is maintained 
· Spa pool rules and safety signage displayed poolside
· Rules to include maximum recommended duration of stay in spa pool of up to 15 minutes
· Visible clock available nearby to help users monitor time
· Users advised not to not put heads below water
· Use of spa pool is restricted to persons over the age of 15
· Persons considered being under the influence of drink/drugs are not permitted to access the swimming pool areas. Must leave the facilities where required
· The use of glass is not permitted
· Bathers are encouraged to shower before entering the spa pool
· Users’ behaviour is monitored and corrected where required
· Opening/closing checks and weekly safety reviews completed, and corrective actions taken where required
· Documented cleaning schedule in place
· Daily opening/closing checks and weekly safety review completed
· Water temperature should never exceed 40°C
· Access to the pool is restricted when the pool is closed


	Swimming pool chemicals

· Exposure to hazardous chemicals such as:
· Chlorine
· Bromine
· Algaecide 
· Cyanuric acid
· pH adjusters
· Spills or leaks of pool chemicals.
· Inadequate ventilation
· Fire hazard from faulty or incorrectly used electrical systems or equipment




	Maintenance-personnel
Compass employees


	Acute/chronic health conditions, from respiratory, dermal or ingestion contact with chemicals as a result of:
· improper handling, use or storage of chemicals
· Spillage or leaks
· Inadequate ventilation

Injuries as a result of explosion or violent chemical reactions due to mixing chemicals.

	· Staff trained in the correct storage and handling of chemicals, and in emergency procedures
· Chemicals only handled by trained competent employees
· Manufacturers guidelines and instructions followed at all times
· Staff provided with required PPE
· PPE stored correctly and replaced as required
· Safety notices clearly displayed in plant room
· Plant room and chemical stores kept locked to restrict access from non-authorised persons
· Chemical Inventory available and complete
· MSDs available for all chemicals
· Chemicals stored in a cool, dry, well-ventilated area, away from heat and sources of ignition
· Chemicals stored in their original containers
· Volumes of chemicals stored in plant room kept to a minimum
· Empty containers disposed of in the correct waste stream
· Physical separation of chemicals where mixing can result in dangerous reactions
· Emergency spill response plan in place and required equipment, including suitable spill kits and PPE available
· Any spillages/leaks addressed immediately.
· All tanks and chemical feed lines clearly labelled to prevent cross-contamination/mixing of chemicals
· Liquid chemical containers stored in a bund for secondary containment
· Each liquid chemical is stored in a separate bund
· Bunds must have a minimum capacity of 110% of the largest container stored in it
· Store acids and chlorine-based products in completely separate, well-ventilated areas
· Dedicated handling and feeding equipment used for each chemical to avoid cross-contamination
· Plant room is adequately ventilated and has sufficient lighting
· Good housekeeping in place to keep plant room clean and tidy, without obstructions
· Fire aid kit, including eye wash station available in the plant room

	Working in the plant room including chlorine filling day tanks and dry acid tanks

· Pool circulation pumps
· Defective pumps and filters
· Electrical systems 
· Pool chemicals including chlorine 
· Wet floors from leaks and condensation
· Obstructions 
· Manual handling
· Fire/explosion
· Corrosion of equipment









	Compass employees
Maintenance personnel

	Entrapment injuries as a result of contact with powerful pool circulation pumps creating strong suction, trapping body parts.

Electrocution or electrical burns due to damaged wiring or faulty equipment.

Exposure to pool chemicals when handling chemicals or as a result of leaks/spillages causing severe eye, skin and respiratory irritation.

Severe injuries/broken or fractured bones/ bruising/cuts/sprains/
strains as a result of slips, trips and falls caused by wet floors, spillages, obstructions etc.

Injuries from explosion or violent chemical reactions caused by mixing of chemicals.

Back and muscle strain as a result of handling heavy containers.

Damage to facilities/equipment as a result of corrosion.

	· Only trained employees to access and use the plant room
· Signage installed clearly designating plant room as a restricted area and hazard warning signs displayed to indicate specific dangers
· Good housekeeping implemented to ensure that area is clear of obstructions, tidy and clean
· Any spillages cleaned up immediately
· Plant room adequately ventilated
· Required PPE including gloves, eye protection, safety boots, aprons, ventilators and gauntlets worn when required
· Manufacturer’s instructions followed when using chemicals
· Dedicated handling and feeding equipment used for each chemical to avoid mixing/cross-contamination
· All feed lines and tanks clearly labelled
· Gas detectors and fire alarms installed in plant room
· Detectors and alarms regularly tested.
· Good manual handling practices implemented, and task specific manual handling risk assessments implemented where required
· Equipment/facilities regularly inspected and any damage including corrosion reported
· Ongoing maintenance of plant room equipment/facilities


	Cleaning swimming pool/spa and surrounds, including scum line:

· Use of cleaning chemicals
· Slips caused by wet/slippery surfaces
· Manual handling 
· Working adjacent to deep water
	Maintenance personnel.

	Irritation/burns/poisoning from contact with cleaning chemicals

Severe or fatal injuries/broken or fractured bones /bruising/cuts/sprains/
Strains/drowning from:
· Slips and falls as a result of wet or slippery surfaces
· Drowning as a result of falls into the pool/spa
Damage to equipment as a result of use of wrong cleaning products.

Manual handling injuries from: 
· Repetitive motion when scrubbing scum line.
· Overreaching.

Explosion or violent chemical reactions as a result of incorrect use of chemicals.

	· Only approved chemicals used
· Employees trained on safe storage and handling of chemicals
· MSD sheets are available
· Staff provided with appropriate PPE for chemicals being used
· PPE is worn when carrying out tasks
· Suitable equipment and chemicals used to avoid damage to surfaces
· Slip-resistant shoes worn at all times
· Where repetitive motions are being carried out staff take breaks or mix up tasks
· Cleaning chemicals are kept away from pool users
· Cleaning tasks are carried out when the pool is closed
· No lone working


	Chlorine Gas Leak
	Compass employees
Maintenance Personnel
Swimmers and guests
	Respiratory and Eye Irritation. Gastrointestinal symptoms:

· inhalation causing irritation in the throat, coughing, wheezing, and shortness of breath. Higher concentrations can lead to pulmonary oedema (fluid in the lungs), which is life-threatening.
· Inhalation causing vomiting and nausea.

	· Employees trained on storage and handling of chlorine chemicals
· Employees trained on safe pool maintenance procedures, equipment operation, and emergency response protocols
· Fixed chlorine gas detectors installed in the plant room to provide early warning of a leak
· Documented Emergency Action Plan (EAP) in place
· All chemicals stored safely 
· Separately marked equipment for chemical decanting
· Qualified First Aiders must be available at all times
 

	Saunas

· Excessive heat exposure
· Excessive heat exposure for persons with existing health conditions or contra-indications including: 
· low or high blood pressure
· cardiovascular issues 
· diabetes
· seizures
· pregnancy
· use of certain medications 
· Excessive heat exposure to persons under the influence of alcohol or drugs 
· Contact with hot surfaces or steam
· Fire hazards due to combustible materials and potential ignition sources, including electrical heaters
· Damaged woodwork
	Guests/visitors
Maintenance-personnel
Compass employees
	Burns/scalds/blister injuries as a result of:
· Direct contact with hot sauna rocks, heaters, or metal surfaces. 
· Heating elements being poorly located.
· Inadequate or inappropriate use of the sauna.

Dehydration, cardiovascular ill health, hypotension/fainting or infections due to:
· Prolonged exposure to high temperatures. 
· Inadequate or inappropriate use of the sauna.
· Inadequate cleaning and hygiene measures.

Fire as a result of ignition of:
· combustible materials in the sauna 

Fungal, bacterial or viral infection as a result of poor hygiene and cleaning.

Splinters or cuts from poorly maintained woodwork.



	· Sauna installed in accordance with the Original Equipment Manufacturers (OEM) instructions
· Sauna regularly inspected and maintained by nominated contractors 
· Suitable location of the heating elements to reduce risk of burns and scalds; where appropriate elements are guarded to prevent contact
· Only coals specified by the manufacturer are used and these are replaced according to the manufacturer’s recommendations
· Temperature gauge fitted inside the sauna to indicate the internal temperature
· Temperature controls are not accessible to users
· Door must have a clear panel to allow safe access and egress
· Emergency panic buttons available inside the sauna
· Clock or timer available to monitor time elapsed
· Regular checks on the internal handle and condition of woodwork are carried out
· Regular checks carried out on sauna cleanliness and health of users
· Drinking water provided in the vicinity
· Daily cleaning and sanitation protocols in place
· Regular checks carried out on cleanliness and health of users
· Sauna is cleaned when it is cool and has been ventilated
· Clear signage on rules and safety precautions, including contra indications, relating to use of sauna clearly displayed
· Users encouraged to shower before and after use
· Use of sauna restricted to persons aged 16 years and over
· Users encouraged to limit sauna time to avoid overheating and dehydration
· Users required to sit on towels while using the sauna
· Persons considered being under the influence of drink/drugs are not permitted to access the swimming pool areas must leave facilities where required
· Qualified First Aiders available at all times the sauna is in use

	Steam rooms

· Excessive heat exposure
· Excessive heat exposure for persons with existing health conditions or contra-indications including: 
· low or high blood pressure
· cardiovascular issues 
· diabetes
· seizures
· pregnancy
· use of certain medications 
· Excessive heat exposure to persons under the influence of alcohol or drugs
· Contact with hot surfaces 
· Bacterial or fungal infection as a result of moist, warm conditions which permit growth of microorganisms
· Slippery surfaces
· Fire hazard from faulty or incorrectly used electrical systems or equipment


	Guests/visitors
Maintenance-personnel
Compass employees
	Burns/scalds/blister injuries as a result of contact with hot surfaces.

Dehydration, cardiovascular ill health, hypotension/fainting or infections due to:
· Prolonged exposure to high temperatures
· Inadequate or inappropriate use of the sauna
· Inadequate cleaning and hygiene measures


· Hygiene, cleaning controls and ventilation not to an appropriate rigorous standard or frequency leading to bacteria growth
Slip, trip or fall injuries caused by wet flooring and surfaces.

	· Steam room installation in accordance with the Original Equipment Manufacturers (OEM) instructions
· Steam room regularly inspected and maintained by nominated contractors
· Suitable location piping and steam outlets to reduce risk of burns and scalds; where appropriate these are guarded to prevent contact
· Temperature gauge fitted inside the steam room to indicate the internal temperature
· Temperature controls are not accessible to users
· Door must have a clear panel to allow safe access and egress
· Emergency panic buttons available inside the steam room
· Clock or timer available to monitor time elapsed
· Regular checks carried out on cleanliness and health of users
· Drinking water provided in the vicinity
· Daily cleaning and sanitation protocols in place
· Steam room is cleaned when it is cool and has been ventilated
· Clear signage on rules and safety precautions, including contra indications, relating to use of steam room clearly displayed
· Users encouraged to shower before and after use
· Use of steam room restricted to persons aged 16 years and over 
· Users advised to take care due to slippery conditions
· Users encouraged to limit steam room time to avoid overheating and dehydration
· Persons considered being under the influence of drink/drugs are not permitted to access the swimming pool areas and are removed where required
· Qualified First Aiders must be available at all times the steam room is in use


	Steam Generator

· Hot steam/hot components/hot water
· Wet floor surfaces
· Cleaning chemicals
· Electrical hazards
· Overheating 
· Mould/bacteria 




 
	Compass employees
Guests	
Maintenance Personnel
	Burns and scolds/cuts and bruising/respiratory, skin and eye irritation/infection/electrocution:


· Direct contact with hot steam, internal components of the steam generator, or hot water used for cleaning can cause serious burns.
· Slippery surfaces leading to slips, trips and fall injuries.
· Irritation from cleaning chemicals 
· Electrocution from poorly maintained electrical equipment.
· Illness from exposure to mould or bacteria build-up.

	· Wear appropriate PPE, such as heat-resistant gloves, eye protection, and appropriate footwear when cleaning the steam generator
· Documented cleaning schedule in place, covering steam generator tank, pipes, and nozzles
· Regular decalcification as required to prevent blockages
· Manufacturer’s guidelines followed for operating, maintaining and cleaning equipment
· Equipment disconnected from the power supply and allowed to cool prior to cleaning or maintenance







	What are the hazards?
	Who might be harmed?
	How might they be harmed?
	What additional actions must be taken to control the risk?

	Additional hazard:
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	Additional hazard:
















	
	
	

	Additional hazard:
















	
	
	

	
Step 3 - Task Specific Control Measures


	Select all the Safety Task Cards which are applicable to the working tasks carried
 out in your unit or business operation by ticking the relevant boxes

	STC
CL 29
	Cleaning swimming pool deck areas
	o
	
	
	o

	STC
LE 02
	Pool vacuum cleaners
	o
	
	
	o

	STC
LE 03
	Pool rope set up and removal
	o
	
	
	o

	STC
CL 01
	General room and office cleaning
	o
	
	
	o

	STC
CL 02
	Cleaning fixtures, walls, partitions, doors, furniture and dispensers
	o
	
	
	o

	STC
CL 03
	Cleaning of ablution areas
	o
	
	
	o

	STC
CL 04
	Cleaning mirrors and glass
	o
	

	STC
CL 05
	Cleaning electrical hand dryers and hair dryers
	o
	

	STC
GE 06 
	Dealing with spillage of body fluids (blood, vomit, faeces and urine
	o
	

	STC
GE 15
	Prevention of medical sharp injuries
	o
	

	STC
GE 04
	Disposal of general waste
	o
	

	STC
GE 03 
	Damp mopping
	o
	

	
	
	o
	

	
	
	o
	

	
	
	o
	

	
	
	o
	

	
	
	o
	

	
	
	o
	

	
	
	o
	

	
	
	o
	

	
	
	o
	

	
	
	o
	

	
	
	o
	

	
	
	o
	

	
	
	o
	



	
Step 4 - Additional Task Specific Control Measures


	Select any additional Safety Task Cards you require by ticking the relevant boxes*
These additional Safety Task Cards are not included in the ‘Safety Task Card Cleaning Services’ pack which you have been provided with but can be downloaded from the HSE website and inserted.
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	o
	
	
	o

	
	
	o
	
	
	o

	
	
	o
	
	
	o
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	o
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	o
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