{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Priority Assessment"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Priority Assessment","index":0,"n_rows":58,"n_cols":9,"rows_kept":58,"cut":false,"hidden":false,"merged":[[57,0,58,6],[57,7,58,8],[40,8,52,8],[42,2,43,2],[42,3,43,6],[42,7,43,7],[44,2,45,2],[44,3,45,6],[44,7,45,7],[46,2,48,2],[46,3,48,6],[46,7,48,7],[40,0,52,0],[27,8,38,8],[31,1,34,1],[35,1,38,1],[29,3,29,6],[30,3,30,6],[31,3,31,6],[27,3,27,6],[28,3,28,6],[27,0,38,0],[27,1,30,1],[35,3,35,6],[36,3,36,6],[37,3,37,6],[38,3,38,6],[10,7,11,7],[12,3,12,6],[39,3,39,6],[14,8,25,8],[18,1,21,1],[22,1,25,1],[16,3,16,6],[17,3,17,6],[18,3,18,6],[19,3,19,6],[20,3,20,6],[21,3,21,6],[22,3,22,6],[25,3,25,6],[24,3,24,6],[26,3,26,6],[53,3,53,6],[55,0,55,7],[56,0,56,7],[50,3,50,6],[51,3,51,6],[52,3,52,6],[49,1,52,1],[49,3,49,6],[54,0,54,7],[0,0,1,8],[13,3,13,6],[14,3,14,6],[15,3,15,6],[23,3,23,6],[2,0,2,8],[3,2,3,4],[3,5,3,6],[3,7,3,8],[5,0,5,1],[5,2,5,6],[4,2,4,4],[14,0,25,0],[14,1,17,1],[6,3,6,6],[6,8,12,8],[4,5,4,6],[4,7,4,8],[6,0,11,0],[6,1,11,1],[40,7,41,7],[32,3,32,6],[33,3,33,6],[34,3,34,6],[40,1,48,1],[40,2,41,2],[40,3,41,6],[8,2,9,2],[8,3,9,6],[8,7,9,7],[10,2,11,2],[10,3,11,6]]}
["                                           FM/HS/F/002/01      Internal Use     May 2018"]
[]
["MANAGEMENT OF ASBESTOS CONTAINING MATERIALS\nPRIORITY ASSESSMENT"]
["Register Number","Asset  ID","Location",null,null,"Use",null,"Material Risk Assesment Score"]
[null,null,null,null,null,null,null,2]
["Assessment factor",null,"Variable(s) selected",null,null,null,null,"Score","Overall Score"]
["ACTIVITY WITHIN AREA","Main type of activity in area",0,"Outdoors",null,null,null,null,"Average Score"]
[null,null,1,"Low disturbance activities (eg office type activity)",null,null,null,1]
[null,null,2,"Periodic disturbance (eg industrial or vehicular activity which may contact ACM's)  "]
[]
[null,null,3,"High levels of disturbance. (eg fire door with asbestos insulating board sheet in constant use)"]
[]
["Secondary activities for area:",null,"As above"]
[null,null,null,"Total :",null,null,null,{"$f":"SUM(H7:H13)","v":1},{"$f":"H14/1","v":1}]
["LIKELIHOOD OF DISTURBANCE","Location",0,"Outdoors",null,null,null,null,"Average Score"]
[null,null,1,"Large rooms or well ventilated areas",null,null,null,1]
[null,null,2,"Rooms up to 100m2"]
[null,null,3,"Confined spaces"]
[null,"Accessibility",0,"Usually inaccessible or unlikely to be disturbed"]
[null,null,1,"Occasionally likely to be disturbed",null,null,null,1]
[null,null,2,"Easily disturbed"]
[null,null,3,"Routinely disturbed"]
[null,"Extent/amount",0,"Small amounts or items (eg strings, gaskets)"]
[null,null,1,"<10m2 to <10m pipe run",null,null,null,1]
[null,null,2,">10m2 to 50m2 or > 10m to < 50m pipe run"]
[null,null,3,">50m2 or 50m pipe run"]
[null,null,null,"Total :",null,null,null,{"$f":"SUM(H15:H26)","v":3},{"$f":"H27/3","v":1}]
["HUMAN EXPOSURE POTENTIAL","Number of Occupants",0,"None",null,null,null,0,"Average Score"]
[null,null,1,"1 to 3"]
[null,null,2,"4 to 10"]
[null,null,3,"> 10"]
[null,"Frequency of use \nof area",0,"Infrequent",null,null,null,0]
[null,null,1,"Monthly"]
[null,null,2,"Weekly"]
[null,null,3,"Daily"]
[null,"Average time area in use ",0,"< 1 hour",null,null,null,0]
[null,null,1,"> 1 to < 3 hours"]
[null,null,2,"> 3 to < 6 hours"]
[null,null,3,"> 6 hours"]
[null,null,null,"Total :",null,null,null,{"$f":"SUM(H28:H39)","v":0},{"$f":"H40/3","v":0}]
["MAINTENANCE ACTIVITY","Type of Maintenance Activity",0,"Minor disturbance(e.g possibility of contact when gaining access) ",null,null,null,0,"Average Score"]
[]
[null,null,1,"Low disturbance (e.g changing light bulbs in asbestos insulating board ceiling)"]
[]
[null,null,2,"Medium disturbance (e.g lifting one or two asbestos insulating board ceiling tiles to access a valve)"]
[]
[null,null,3,"High levels of disturbance. (eg removing a number of asbestos board ceiling tiles to replace a valve or for recabling)"]
[]
[]
[null,"Frequency of Maintenance Activity",0,"ACM unlikely to be disturbed for maintenance",null,null,null,0]
[null,null,1,"< 1 per year"]
[null,null,2,"> 1 per year"]
[null,null,3,"> 1 per month"]
[null,null,null,"Total :",null,null,null,{"$f":"SUM(H41:H53)","v":0},{"$f":"H54/2","v":0}]
["Total priority assessment score :",null,null,null,null,null,null,null,{"$f":"I14+I27+I40+I54","v":2}]
["   Material assessment score ( supplied by surveyor ) :",null,null,null,null,null,null,null,{"$f":"H5","v":2}]
["Total of material and priority assessment scores :",null,null,null,null,null,null,null,{"$f":"I55+I56","v":4}]
["Priority Assessment Author :"]